CORRW ASCII
CorrTest for Windows: SN CS310M2108624  V6.5.1230.3  V3.0.210914.1
ID_PotDynamic
Data:2025-05-23   Time:15:41:24
ExpParmas:ExpType=ID_PotDynamic&-&InitE=-0.015&-&MidEOne=-0.1&-&MidETwo=-0.1&-&FinalE=0.015&-&ScanRate=0.167&-&InitEVsOcp=vsOCP&-&MidEOneVsOcp=vsOCP&-&MidETwoVsOcp=vsOCP&-&FinalEVsOcp=vsOCP&-&MidEOneEnable=False&-&MidETwoEnable=False&-&ScanStopEnable=False&-&ScanReverse=False&-&MaxCurrent=2&-&MinCurrent=-2&-&ScanRateUnit=0&-&IsReve=False&-&FileName=C:\Users\vp2039\Desktop\thesis\Electrochemical\HIPed_Stellite1_EIS_LPR\test_ReStart_ReStart_ReStart.cor&-&FilePath=C:\Users\vp2039\Desktop\thesis\Electrochemical\HIPed_Stellite1_EIS_LPR\test_ReStart_ReStart_ReStart.cor&-&Comment=&-&IsFrq=False&-&SampleInter=0.5&-&SampleFrq=2&-&Number=0&-&EnableAxisType=True&-&AxisType=EvsLogi&-&OcpValue=-0.259446442127228&-&IsStopEvent=False&-&Frq=0.334&-&ExpTime=179.6406&-&DevParam=VoltRange=2&|&EnableWaitSecond=True&|&IsWaitSecond=True&|&WaitSecondEx=5&|&IsCurrAutoRange=True&|&IsVoltAutoRange=True&|&OnlyInc=True&|&AutoMinCurrRange=8&|&OnlyIncE=True&|&AutoMinVoltRange=2&|&IsIR=False&|&IrModeEx=2&|&IrValue=5.0731&|&IsVoltRule=True&|&IsCurrRule=True&|&XiaoboqiEnable=True&|&Xianboqi=True&|&ManualCurRange=3&|&FilterCap=2&|&IsContainsUnit=False&|&LowFilter=True&|&OneKHzFilter=True&|&DigitalSmoothModeEx=1&|&DigitLPFCount=5&|&LineFre=0&|&IsIgnoreFre=True&|&OcpState=False&|&DeltaMaxOcp=10&|&WEMode=0&|&GroundingMode=0&|&IsLowSpeedFilter=False&|&IsEnableCY=False&|&OutputMode=0&|&OutputTime=100&-&CellParam=Area=2&|&AreaMode=0&|&Density=7.8&|&Dangliang=28&|&Type=2&|&REValue=0.241&|&Temp=25&|&Stern=26&|&Enable=True&|&IsGetTemp=False&|&EnableSpeed=False&|&RotatingSpeed=3200&-&ExpType=ID_PotDynamic&-&Issampling=True&-&EnablePause=True&-&EnablePolar=True&-&Cycles=1&-&DefaultE=0&-&DefaultI=0,ExpInfo:Init E(V):-0.015 vs OCP.,Final E(V):0.015 vs OCP.,Scan Rate(mV/s):0.167,Freq(Hz):0.334
Open Circuit Potential (V):-0.25945

Temperature(℃):   25
  Begin Information:            Cell Information
      Surface Area:           2
      Density:                7.8
      Weight:                 28
      Polarity:               0
      PolarityI:              0
      Corrosion Unit Type:    1
      Reference Type:         2
      Reference Potential:    0.241
      Reference User-Defined: 2
      Stern-Geary:            26
  End Information:              Cell Information
  Begin Experiment:
      Axes Type:              4
  End Experiment:
E(V)		i(A/cm²)		T(s)
End Comments